IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project nummer"
Time stamp: "2018-04-26T11:13:19"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160720_1515(x64) - Exporter 17.0.501.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "DDA" of Organization (no name given)
  Owner history of Person "DDA" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1524464673 (2018-04-23T06:24:33Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project nummer" | long name "Project omschrijving" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "V00" | long name "V00" | elevation 0.
        contains 1 element
          1 x IFCBOILER | type IFCBOILERTYPE "310-650" | object type "310-650" | names: "HC_Connector Set_MEPcontent_Remeha_Gas 310-650 Eco Pro_Heat Exchanger_INT-EN:310-650:1312105" | material: materials ("Color RGB 152-152-152", "Color RGB 230-194-087", "Color RGB 000-255-255", "Color RGB 146-184-143", "Color RGB 126-162-254", "Color RGB 164-140-255", "Color RGB 180-180-180", "Color RGB 192-192-192", "Color RGB 163-163-175", "Color RGB 040-040-040", "Color RGB 112-104-107") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical, Other

Types
  IFCBOILERTYPE "310-650" | WATER | 1 occurrence | material: materials ("Color RGB 152-152-152", "Color RGB 230-194-087", "Color RGB 000-255-255", "Color RGB 146-184-143", "Color RGB 126-162-254", "Color RGB 164-140-255", "Color RGB 180-180-180", "Color RGB 192-192-192", "Color RGB 163-163-175", "Color RGB 040-040-040", "Color RGB 112-104-107") | property sets: Dimensions, Identity Data, Materials and Finishes, Mechanical, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Klant naam" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Aanvraag datum" (IFCTEXT)
    Project Name = "Project omschrijving" (IFCTEXT)
    Project Number = "Project nummer" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBOILER)
    Angle 3 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Bottom Connector Front Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Connector Horizontal Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Connector Vertical Offset = 357.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Connector Offset 1 = 340.99 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Offset 2 = 601.21 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Offset 3 = 1609.53 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Offset 4 = 325.98 (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "HC_Connector Set_MEPcontent_Remeha_Gas 310-650 Eco Pro_Heat Exchanger_INT-EN: 310-650" (IFCLABEL)
    Family and Type = "HC_Connector Set_MEPcontent_Remeha_Gas 310-650 Eco Pro_Heat Exchanger_INT-EN: 310-650" (IFCLABEL)
    Flange Left = FALSE (IFCBOOLEAN)
    Flange Right = FALSE (IFCBOOLEAN)
    Heat Exchanger Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Horizontal Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Insertion Point Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Insetion Point 2 Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left = TRUE (IFCBOOLEAN)
    Left Handle = TRUE (IFCBOOLEAN)
    Left Heat Exchanger Connector = TRUE (IFCBOOLEAN)
    Offset Length = 852. (IFCLENGTHMEASURE) [MILLI METRE]
    Position Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Right = FALSE (IFCBOOLEAN)
    Right Handle = FALSE (IFCBOOLEAN)
    Service Space Offset = 812. (IFCLENGTHMEASURE) [MILLI METRE]
    Straight Condition = FALSE (IFCBOOLEAN)
    Top Connector Front Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Connector Vertical Offset = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Connector Set_MEPcontent_Remeha_Gas 310-650 Eco Pro_Heat Exchanger_INT-EN: 310-650" (IFCLABEL)
    Type Id = "HC_Connector Set_MEPcontent_Remeha_Gas 310-650 Eco Pro_Heat Exchanger_INT-EN: 310-650" (IFCLABEL)
    Vertical Offset = 852. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Connector Set_MEPcontent_Remeha_Gas 310-650 Eco Pro_Heat Exchanger_INT-EN" (IFCTEXT)
    Heat Exchanger Depth = 562. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Offset = 774.32 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBOILER)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "V00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Description = "Connector set with heat exchanger" (IFCTEXT)
    Article Type = "310-650" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Connector set with heat exchanger" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC011397" (IFCTEXT)
    Family Version = "11.14" (IFCTEXT)
    GTIN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "CONNECTOR_SET" (IFCTEXT)
    Manufacturer = "Remeha" (IFCTEXT)
    Manufacturer Art. No. = "7674637" (IFCTEXT)
    Manufacturer URL = "http://www.remeha.nl" (IFCTEXT)
    Model = "310-650" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "Remeha" (IFCTEXT)
    Revit Version = "2017" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "310-650" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBOILER)
    Manufacturer = "Remeha" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBOILER)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCBOILER)
    Angle 1 = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Angle 2 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Area = 13.1324716121869 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.472361945922428 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 963.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1155.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Diameter = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Diameter = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Diameter = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Diameter = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 1723. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBOILER)
    Hydronic Return 1 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return 2 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply 1 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply 2 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Hydronic Return,Hydronic Supply,Hydronic Return" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Flow Rate (l/s (dt 20°C)) = 0.00777 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Heat Exchanger Power = 650999.998989398 (IFCPOWERMEASURE) [WATT]
    Max Operating Pressure = 30 (IFCINTEGER)
    Primary T In = 85 (IFCINTEGER)
    Primary T Out = 65 (IFCINTEGER)
    Secondary T In = 60 (IFCINTEGER)
    Secondary T Out = 80 (IFCINTEGER)
  Phasing | properties | on 1 object (1 IFCBOILER)
    Phase Created = "4. Plan over 10 jaar" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBOILER)
    Back Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Front Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Mat = FALSE (IFCBOOLEAN)
    Left Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perpendicular Left = FALSE (IFCBOOLEAN)
    Perpendicular Right = FALSE (IFCBOOLEAN)
    Right Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Safety Bar = TRUE (IFCBOOLEAN)
    Service Space = FALSE (IFCBOOLEAN)
    Top Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    Connection Color = "Color RGB 230-194-087" (IFCLABEL)