IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project nummer"
Time stamp: "2019-10-30T14:53:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "FCiofle" of Organization (no name given)
  Owner history of Person "FCiofle" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1571734251 (2019-10-22T08:50:51Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project nummer" | long name "Project omschrijving" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "V00" | long name "V00" | elevation 0.
        contains 1 element
          1 x IFCBOILER | type IFCBOILERTYPE "2x AMC 45 with Concentric Connection 125" | object type "2x AMC 45 with Concentric Connection 125" | names: "HC_Boiler_MEPcontent_De Dietrich Thermique_Cascade Wall-Mounted 2_Evodens Pro_AMC 45-115_INT-EN:2x AMC 45 with Concentric Connection 125:1390897" | material: materials ("Color RGB 149-149-149", "Color RGB 202-154-058", "Color RGB 168-168-168", "Color RGB 229-190-001", "Color RGB 219-015-004", "Color RGB 039-039-039", "Color RGB 017-187-251", "Color RGB 120-120-120", "Color RGB 246-246-246") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads, Identity Data, Mechanical

Types
  IFCBOILERTYPE "2x AMC 45 with Concentric Connection 125" | WATER | 1 occurrence | material: materials ("Color RGB 149-149-149", "Color RGB 202-154-058", "Color RGB 168-168-168", "Color RGB 229-190-001", "Color RGB 219-015-004", "Color RGB 039-039-039", "Color RGB 017-187-251", "Color RGB 120-120-120", "Color RGB 246-246-246") | property sets: Dimensions, Electrical, Identity Data, Materials and Finishes, Mechanical - Flow, Mechanical - Loads

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Klant naam" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Aanvraag datum" (IFCTEXT)
    Project Name = "Project omschrijving" (IFCTEXT)
    Project Number = "Project nummer" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBOILER)
    Category = "Mechanical Equipment" (IFCLABEL)
    Connections Width Offset = 1608. (IFCLENGTHMEASURE) [MILLI METRE]
    Connections on Right = FALSE (IFCBOOLEAN)
    Connectors Angle = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Distributor Left Offset = 531. (IFCLENGTHMEASURE) [MILLI METRE]
    Distributor Right Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "HC_Boiler_MEPcontent_De Dietrich Thermique_Cascade Wall-Mounted 2_Evodens Pro_AMC 45-115_INT-EN: 2x AMC 45 with Concentric Connection 125" (IFCLABEL)
    Family and Type = "HC_Boiler_MEPcontent_De Dietrich Thermique_Cascade Wall-Mounted 2_Evodens Pro_AMC 45-115_INT-EN: 2x AMC 45 with Concentric Connection 125" (IFCLABEL)
    Front Clearance Safe = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Width Offset = 1431. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 277. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Counter Flange = FALSE (IFCBOOLEAN)
    Left Counter Flange Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance Safe = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Counter Flange = FALSE (IFCBOOLEAN)
    Right Counter Flange Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Boiler_MEPcontent_De Dietrich Thermique_Cascade Wall-Mounted 2_Evodens Pro_AMC 45-115_INT-EN: 2x AMC 45 with Concentric Connection 125" (IFCLABEL)
    Type Id = "HC_Boiler_MEPcontent_De Dietrich Thermique_Cascade Wall-Mounted 2_Evodens Pro_AMC 45-115_INT-EN: 2x AMC 45 with Concentric Connection 125" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Boiler_MEPcontent_De Dietrich Thermique_Cascade Wall-Mounted 2_Evodens Pro_AMC 45-115_INT-EN" (IFCTEXT)
    Gas Height Offset = 268. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Height Offset = 210. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Height Offset = 540. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "AMC 45" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBOILER)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Design Option = "Main Model" (IFCTEXT)
    Name = "V00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Type = "2x AMC 45 with Concentric Connection 125" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "12.07" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Gas condensing boiler cascade system" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC011396" (IFCTEXT)
    Family Version = "12.05" (IFCTEXT)
    GLN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "BOILER" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer URL = "http://international.dedietrich-heating.com/" (IFCTEXT)
    Model = "2x AMC 45 with Concentric Connection 125" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Revit Version = "2017" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "2x AMC 45 with Concentric Connection 125" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBOILER)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBOILER)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCBOILER)
    Area = 11.8893396263075 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.430651993911247 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 515. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Gas Diameter = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1576. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Diameter = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 1062. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBOILER)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Mechanical | properties | on 1 object (1 IFCBOILER)
    System Classification = "Hydronic Return,Hydronic Supply,Undefined,Power,Supply Air,Exhaust Air,Supply Air,Exhaust Air,Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCBOILER)
    Drain Fixture Units 1 = 0. (IFCREAL)
    Drain Fixture Units 2 = 0. (IFCREAL)
    Flue Gas Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flue Gas Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 type object
    Nominal Water Flow = 0.00096 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCBOILER)
    Phase Created = "4. Plan over 10 jaar" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBOILER)
    Connections on Left = TRUE (IFCBOOLEAN)
    Counter Flange = FALSE (IFCBOOLEAN)
    Front Clearance = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Service Space = FALSE (IFCBOOLEAN)
    Top Clearance = 400. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Phase = 1 (IFCINTEGER)
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Grey = "Color RGB 149-149-149" (IFCLABEL)
  Mechanical - Loads | properties | on 1 type object
    Nominal Output (kW) = 81.6 (IFCREAL)
  Text | properties | on 1 type object
    Article Description = "Gas condensing boiler cascade system" (IFCTEXT)
    GTIN = "" (IFCTEXT)
    Manufacturer Art. No. = "LW.0080kW.2000" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)