IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2016-02-02T14:29:22"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 2014.0.2013.1024 - Default UI"
Application: "Autodesk Revit MEP 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit MEP 2014 (ENU)"

People and organizations
  Person "CN" of Organization (no name given)
  Owner history of Person "CN" of Organization (no name given) | application "Autodesk Revit MEP 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit MEP 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "PMC-M 20-28 MI" | object type "PMC-M 20-28 MI" | names: "HC_Boiler_MEPcontent_De Dietrich Thermique_PMC-X:PMC-M 20-28 MI:669748" | material: materials ("Color RAL 9016", "Color RAL 7040") | property sets: Identity Data, Text, Phasing, Visibility, Electrical - Loads, Mechanical

Types
  IFCBOILERTYPE "PMC-M 20-28 MI" | element type "PMC-M 20-28 MI" | WATER | 1 occurrence | material: materials ("Color RAL 9016", "Color RAL 7040")

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Function Code = "" (IFCTEXT)
    Mark = "16" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Article Description = "Gas condensing boiler" (IFCTEXT)
    Article Type = "PMC-M 20-28 MI" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Content Supplier URL = "www.mepcontent.eu" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Gas condensing boiler" (IFCTEXT)
    EMCS Version = "2.0" (IFCTEXT)
    ETIM Article Class = "EC011396" (IFCTEXT)
    Family Version = "10.06" (IFCTEXT)
    GTIN = "3661238576391" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    Language = "" (IFCTEXT)
    MEPcontent Class = "BOILER" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer Art. No. = "7602625" (IFCTEXT)
    Manufacturer URL = "http://www.dedietrich-thermique.fr/produits/gammes_de_produits/chaudieres_murales/gaz_condensation_pmcx" (IFCTEXT)
    Model = "PMC-M 20-28 MI" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)
    Revit Version = "2014" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Text | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Concentric Connection = "60/100" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Show Service Area = FALSE (IFCBOOLEAN)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Apparent Load = 0. (IFCREAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Power = 613.542893752454 (IFCREAL)
    Voltage = 2475.69939584324 (IFCREAL)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Domestic Cold Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Fixture Units Drain = 0. (IFCREAL)
    Flue Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Supply Air,Hydronic Supply,Domestic Hot Water,Other,Domestic Cold Water,Hydronic Return,Power,Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Domestic Hot Water Maximum Flow (at ΔT=30K – EN13203-1) = 0.00023 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Minimal Power = 65659.8535419293 (IFCREAL)
    Nominal Power = 224965.727709233 (IFCREAL)
    Volume = 0.0565034667543817 (IFCREAL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Depth = 363.99557376 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 553.99326336 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 367.99552512 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 364. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Base Offset = 250.000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Diameter = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Gas Diameter = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Gas Radius = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Radius = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Materials and Finishes | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Glass = "Color RGB 218-227-224" (IFCLABEL)
    Grey = "Color RAL 7040" (IFCLABEL)
    White = "Color RAL 9016" (IFCLABEL)