IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project nummer"
Time stamp: "2018-10-08T14:47:50"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160720_1515(x64) - Exporter 17.0.501.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "FCiofle" of Organization (no name given)
  Owner history of Person "FCiofle" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1538987414 (2018-10-08T08:30:14Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project nummer" | long name "Project omschrijving" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "V00" | long name "V00" | elevation 0.
        contains 1 element
          1 x IFCBOILER | type IFCBOILERTYPE "27 TR-2 H" | object type "27 TR-2 H" | names: "HC_Boiler_MEPcontent_De Dietrich Thermique_HPI-H Evolution_FR-EN:27 TR-2 H:1312058" | material: materials ("Color RGB 150-150-150", "Color RGB 187-080-046", "Color RGB 246-246-246", "Color RGB 208-181-070") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads, Identity Data, Mechanical

Types
  IFCBOILERTYPE "27 TR-2 H" | WATER | 1 occurrence | material: materials ("Color RGB 150-150-150", "Color RGB 187-080-046", "Color RGB 246-246-246", "Color RGB 208-181-070") | property sets: Dimensions, Electrical, Electrical Engineering, Identity Data, Materials and Finishes, Mechanical

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Klant naam" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Aanvraag datum" (IFCTEXT)
    Project Name = "Project omschrijving" (IFCTEXT)
    Project Number = "Project nummer" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBOILER)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Boiler_MEPcontent_De Dietrich Thermique_HPI-H Evolution_FR-EN: 27 TR-2 H" (IFCLABEL)
    Family and Type = "HC_Boiler_MEPcontent_De Dietrich Thermique_HPI-H Evolution_FR-EN: 27 TR-2 H" (IFCLABEL)
    Type = "HC_Boiler_MEPcontent_De Dietrich Thermique_HPI-H Evolution_FR-EN: 27 TR-2 H" (IFCLABEL)
    Type Id = "HC_Boiler_MEPcontent_De Dietrich Thermique_HPI-H Evolution_FR-EN: 27 TR-2 H" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    D1 = 37.2 (IFCLENGTHMEASURE) [MILLI METRE]
    D2 = 24.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Family Name = "HC_Boiler_MEPcontent_De Dietrich Thermique_HPI-H Evolution_FR-EN" (IFCTEXT)
    Gas Nominal Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Outer Diameter = 33.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Nominal Diameter = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Liquid Outer Diameter = 21.3 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBOILER)
    Design Option = "Main Model" (IFCTEXT)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Design Option = "Main Model" (IFCTEXT)
    Name = "V00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Type = "HPI 27 TR-2 H" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "11.19" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Boiler indoor unit MIT-IN-2 H" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC011396" (IFCTEXT)
    Family Version = "11.19" (IFCTEXT)
    GLN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "BOILER" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer URL = "https://www.dedietrich-thermique.fr/" (IFCTEXT)
    Model = "HPI 27 TR-2 H" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Revit Version = "2017" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "27 TR-2 H" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBOILER)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBOILER)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCBOILER)
    Area = 8.81060462906738 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 3.62172009880448 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 498. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Cold Water Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 1 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return 2 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 1 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply 2 Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Refrigerant Gas Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Refrigerant Liquid Diameter = 12.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCBOILER)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Mechanical | properties | on 1 object (1 IFCBOILER)
    System Classification = "Power,Sanitary,Hydronic Return,Hydronic Supply,Domestic Cold Water,Domestic Hot Water,Hydronic Return,Hydronic Supply,Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Cooling Capacity (+ 35 °C to+ 18 °C) = 238958.81088 (IFCREAL)
    Cooling Capacity (+ 35 °C to+ 7 °C) = 125937.75168 (IFCREAL)
    Heating Capacity (+ 2 °C to+ 35 °C) = 158229.48288 (IFCREAL)
    Heating Capacity (+ 7 °C to+ 35 °C) = 262639.41376 (IFCREAL)
    Heating Capacity (- 7 °C to+ 35 °C) = 148541.96352 (IFCREAL)
    Volume = 40. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Mechanical - Flow | properties | on 1 object (1 IFCBOILER)
    Domestic Cold Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Drain Fixture Units = 0. (IFCREAL)
    Hydronic Return 1 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return 2 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply 1 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply 2 Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Refrigerant Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Refrigerant Liquid Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 type object
    Nominal Air Flow = 2.333 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Nominal Water Flow = 0.00128 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCBOILER)
    Phase Created = "4. Plan over 10 jaar" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBOILER)
    Service Space = FALSE (IFCBOOLEAN)
  Visibility | properties | on 1 type object
    Bottom Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Front Clearance = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Absorbed Electrical Power (+ 35 °C to+ 18 °C) kWe = 5.84 (IFCREAL)
    Absorbed Electrical Power (+ 7 °C to+ 35 °C) kWe = 6.25 (IFCREAL)
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 3 (IFCINTEGER)
    Seasonal Energy Efficiency Etas (%) = "115" (IFCTEXT)
    Voltage = 399.999999379046 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical Engineering | properties | on 1 type object
    Nominal Intensity = 9.86 (IFCELECTRICCURRENTMEASURE) [AMPERE]
  Materials and Finishes | properties | on 1 type object
    Light Grey = "Color RGB 150-150-150" (IFCLABEL)
    Pipes Material = "Color RGB 187-080-046" (IFCLABEL)
    White = "Color RGB 246-246-246" (IFCLABEL)
    Yellow = "Color RGB 208-181-070" (IFCLABEL)
  Mechanical - Loads | properties | on 1 type object
    Cooling COP (+ 35 °C to + 18 °C) = 3.8 (IFCREAL)
    Cooling COP (+ 35 °C to + 7 °C) = 2.9 (IFCREAL)
    Heating COP (+ 2°C to+ 35 °C) = 3.13 (IFCREAL)
    Heating COP (+ 7 °C to+ 35 °C) = 3.9 (IFCREAL)
    Heating COP (- 7 °C to+ 35 °C) = 2.26 (IFCREAL)
    Indoor Unit Weight = 72. (IFCREAL)
    Maximum Preloaded Length = 30000. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Pressure at Nominal Debit (mbar) = 0. (IFCREAL)
    Outdoor Unit Weight = 141. (IFCREAL)
    Refrigerant R 410A = 7.7 (IFCREAL)
    Sound Pressure Level Indoor Unit dB(A) = 43.4 (IFCREAL)
    Sound Pressure Level Outdoor Unit dB(A) = 77. (IFCREAL)
  Text | properties | on 1 type object
    Article Description = "Boiler indoor unit MIT-IN-2 H" (IFCTEXT)
    GTIN = "3661238589599" (IFCTEXT)
    Manufacturer Art. No. = "7609936" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)