IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2019-01-29T16:39:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160720_1515(x64) - Exporter 17.0.501.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "EComsa" of Organization (no name given)
  Owner history of Person "EComsa" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBOILER | type IFCBOILERTYPE "MCA 160" | object type "MCA 160" | names: "HC_Boiler_MEPcontent_De Dietrich Thermique_Innovens PRO_MCA 160_FR-EN:MCA 160:6086" | material: materials ("Color RGB 246-246-246", "Color RGB 127-118-121", "Color RGB 163-163-163") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical, Identity Data, Mechanical

Types
  IFCBOILERTYPE "MCA 160" | WATER | 1 occurrence | material: materials ("Color RGB 246-246-246", "Color RGB 127-118-121", "Color RGB 163-163-163") | property sets: Dimensions, Electrical, Identity Data, Materials and Finishes, Mechanical, Mechanical - Flow

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBOILER)
    Bottom Clearance Safe = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Boiler_MEPcontent_De Dietrich Thermique_Innovens PRO_MCA 160_FR-EN: MCA 160" (IFCLABEL)
    Family and Type = "HC_Boiler_MEPcontent_De Dietrich Thermique_Innovens PRO_MCA 160_FR-EN: MCA 160" (IFCLABEL)
    Front Clearance Safe = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance Safe = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Boiler_MEPcontent_De Dietrich Thermique_Innovens PRO_MCA 160_FR-EN: MCA 160" (IFCLABEL)
    Type Id = "HC_Boiler_MEPcontent_De Dietrich Thermique_Innovens PRO_MCA 160_FR-EN: MCA 160" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Boiler_MEPcontent_De Dietrich Thermique_Innovens PRO_MCA 160_FR-EN" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBOILER)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBOILER)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBOILER)
    Area = 9.19812825872206 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.368855825608505 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Drain Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Gas Diameter = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1045. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Diameter = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 602. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical | properties | on 1 object (1 IFCBOILER)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Electrical | properties | on 1 type object
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Identity Data | properties | on 1 object (1 IFCBOILER)
    Function Code = "" (IFCTEXT)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Article Description = "Gas condensing boiler" (IFCTEXT)
    Article Type = "MCA 160" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "11.25" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Gas condensing boiler" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC011396" (IFCTEXT)
    Family Version = "11.25" (IFCTEXT)
    GLN = "" (IFCTEXT)
    GTIN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "BOILER" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer Art. No. = "" (IFCTEXT)
    Manufacturer URL = "https://www.dedietrich-thermique.fr/nos-produits/collectif-chaudieres-et-accessoires/innovens-pro/" (IFCTEXT)
    Model = "MCA 160" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)
    Revit Version = "2017" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "MCA 160" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBOILER)
    Fixture Units Drain = 0. (IFCREAL)
    System Classification = "Hydronic Return,Sanitary,Hydronic Supply,Other,Supply Air,Other,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Maximal Nominal Power ( 50/30°C) = 1739447.92064 (IFCREAL)
    Maximal Nominal Power ( 80/60°C) = 1637190.77184 (IFCREAL)
    Minimal Nominal Power ( 50/30°C) = 373507.69088 (IFCREAL)
    Minimal Nominal Power ( 80/60°C) = 339063.1776 (IFCREAL)
    Volume = 0.017 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Mechanical - Flow | properties | on 1 object (1 IFCBOILER)
    Flue Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical - Flow | properties | on 1 type object
    Nominal Water Flow = 0.0635664000986795 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCBOILER)
    Phase Created = "New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBOILER)
    Bottom Clearance = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Front Clearance = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Service Space = FALSE (IFCBOOLEAN)
    Top Clearance = 500. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 type object
    Grey = "Color RGB 127-118-121" (IFCLABEL)
    Light Grey = "Color RGB 163-163-163" (IFCLABEL)
    White = "Color RGB 246-246-246" (IFCLABEL)
  Mechanical - Loads | properties | on 1 type object
    Maximum Pressure at Nominal Debit (mbar) = 170. (IFCREAL)
    Unit Weight (kg) = 147. (IFCREAL)