IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project nummer"
Time stamp: "2018-10-08T11:49:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160720_1515(x64) - Exporter 17.0.501.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "FCiofle" of Organization (no name given)
  Owner history of Person "FCiofle" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1538987414 (2018-10-08T08:30:14Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project nummer" | long name "Project omschrijving" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "V00" | long name "V00" | elevation 0.
        contains 1 element
          1 x IFCPUMP | type IFCPUMPTYPE "AWHP 16 MR-2" | object type "AWHP 16 MR-2" | names: "HC_Heat Pump_MEPcontent_De Dietrich Thermique_FR-EN:AWHP 16 MR-2:1339274" | material: materials ("Color RGB 173-175-175", "Color RGB 216-216-216", "Color RGB 100-100-100") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads, Identity Data, Mechanical

Types
  IFCPUMPTYPE "AWHP 16 MR-2" | 1 occurrence | material: materials ("Color RGB 173-175-175", "Color RGB 216-216-216", "Color RGB 100-100-100") | property sets: Dimensions, Electrical, Identity Data, Materials and Finishes, Other, Text

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Klant naam" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Aanvraag datum" (IFCTEXT)
    Project Name = "Project omschrijving" (IFCTEXT)
    Project Number = "Project nummer" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCPUMP)
    Back Clearance Safe = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Heat Pump_MEPcontent_De Dietrich Thermique_FR-EN: AWHP 16 MR-2" (IFCLABEL)
    Family and Type = "HC_Heat Pump_MEPcontent_De Dietrich Thermique_FR-EN: AWHP 16 MR-2" (IFCLABEL)
    Front Clearance Safe = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance Safe = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance Safe = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Clearance Safe = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "HC_Heat Pump_MEPcontent_De Dietrich Thermique_FR-EN: AWHP 16 MR-2" (IFCLABEL)
    Type Id = "HC_Heat Pump_MEPcontent_De Dietrich Thermique_FR-EN: AWHP 16 MR-2" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Heat Pump_MEPcontent_De Dietrich Thermique_FR-EN" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Design Option = "Main Model" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCPUMP)
    Design Option = "Main Model" (IFCTEXT)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "V00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Type = "AWHP 16 MR-2" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "11.19" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Heat pump outdoor unit" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC001213" (IFCTEXT)
    Family Version = "11.19" (IFCTEXT)
    GLN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "HEATPUMP" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer URL = "https://www.dedietrich-thermique.fr/" (IFCTEXT)
    Model = "AWHP 16 MR-2" (IFCTEXT)
    OmniClass Number = "23.75.10.21" (IFCTEXT)
    OmniClass Title = "Heat Pumps" (IFCTEXT)
    Revit Version = "2017" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "AWHP 16 MR-2" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCPUMP)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCPUMP)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCPUMP)
    Area = 13.3894359509937 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 6.55403581291607 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Depth = 330. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 33. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1350. (IFCLENGTHMEASURE) [MILLI METRE]
    Refrigerant Gas Diameter = 15.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Refrigerant Liquid Diameter = 9.53 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 950. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCPUMP)
    Power = 3360. (IFCPOWERMEASURE) [WATT]
  Mechanical | properties | on 1 object (1 IFCPUMP)
    System Classification = "Undefined,Power,Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCPUMP)
    Drain Fixture Units = 0. (IFCREAL)
    Refrigerant Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Refrigerant Liquid Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCPUMP)
    Phase Created = "4. Plan over 10 jaar" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCPUMP)
    Back Clearance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Front Clearance = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Clearance = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Service Space = FALSE (IFCBOOLEAN)
    Top Clearance = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Hertz = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Voltage = 229.999999642952 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Grey = "Color RGB 100-100-100" (IFCLABEL)
    Light Grey = "Color RGB 173-175-175" (IFCLABEL)
    White = "Color RGB 216-216-216" (IFCLABEL)
  Text | properties | on 1 type object
    Article Description = "Heat pump outdoor unit" (IFCTEXT)
    GTIN = "3661238589551" (IFCTEXT)
    Manufacturer Art. No. = "7609929" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)