IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2020-10-15T13:26:09"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Default UI"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "PRoman1" of Organization (no name given)
  Owner history of Person "PRoman1" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1601457812 (2020-09-30T09:23:32Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "F00" | long name "F00" | elevation 0.
        contains 1 element
          1 x IFCBOILER | type IFCBOILERTYPE "350 VG" | object type "350 VG" | names: "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C 340 5-7_Left_FR-FR:350 VG:1377517" | material: materials ("Color RGB 165-173-178", "Color RAL 7016", "Color RGB 219-219-219", "Color RGB 145-145-145", "Color RGB 075-186-252", "Color RGB 255-255-000", "Color RAL 2002") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical - Loads, Identity Data, Mechanical

Types
  IFCBOILERTYPE "350 VG" | 1 occurrence | material: materials ("Color RGB 165-173-178", "Color RAL 7016", "Color RGB 219-219-219", "Color RGB 145-145-145", "Color RGB 075-186-252", "Color RGB 255-255-000", "Color RAL 2002") | property sets: Dimensions, Electrical, Identity Data, Materials and Finishes, Mechanical, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBOILER)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBOILER)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCBOILER)
    Area = 20.7440260100866 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.27500096229357 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Air Inlet Connection Size = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Condensate Drain Size = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Connection Size = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Flow and Return Connection Size = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Connection Size = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Fuel Connection Size = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1550. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Length = 1862. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 707. (IFCLENGTHMEASURE) [MILLI METRE]
    Safety Valve Connection Size = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Safety Valve Diameter = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
  Electrical - Loads | properties | on 1 object (1 IFCBOILER)
    Power = 0. (IFCPOWERMEASURE) [WATT]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBOILER)
    Design Option = "Main Model" (IFCTEXT)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Design Option = "Main Model" (IFCTEXT)
    Name = "F00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Description = "C 340 - 350 VG" (IFCTEXT)
    Article Type = "350 VG" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "12.19" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Trimble Europe BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "C 340 - 350 VG" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC010232" (IFCTEXT)
    Family Version = "12.18" (IFCTEXT)
    GLN = "8713809000004" (IFCTEXT)
    GTIN = "8713809338831" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "BOILER_CONDENSATE_FLOW" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer Art. No. = "7769070" (IFCTEXT)
    Manufacturer URL = "http://pro.dedietrich-thermique.fr/fr/site_pro" (IFCTEXT)
    Model = "350 VG" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)
    Revit Version = "2018" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "350 VG" (IFCTEXT)
    URL = "https://mep.trimble.com" (IFCTEXT)
    Watermarked By = "https://mep.trimble.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBOILER)
    System Classification = "Other,Sanitary,Supply Air,Other,Power,Hydronic Supply,Hydronic Return" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Classification = "None" (IFCIDENTIFIER)
  Mechanical - Flow | properties | on 1 object (1 IFCBOILER)
    Drain Fixture Units = 0. (IFCREAL)
    Flue Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Gas Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Return Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hydronic Supply Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Supply Air Flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Client Name" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Project Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBOILER)
    Category = "Mechanical Equipment" (IFCLABEL)
    Connector Placement = 115. (IFCLENGTHMEASURE) [MILLI METRE]
    Family = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C 340 5-7_Left_FR-FR: 350 VG" (IFCLABEL)
    Family and Type = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C 340 5-7_Left_FR-FR: 350 VG" (IFCLABEL)
    Type = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C 340 5-7_Left_FR-FR: 350 VG" (IFCLABEL)
    Type Id = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C 340 5-7_Left_FR-FR: 350 VG" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Access Clearance Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Access Clearance Front = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Access Clearance Left = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Access Clearance Rear = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Access Clearance Right = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Access Clearance Top = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "HC_Boiler_Condensate Flow_MEPcontent_De Dietrich Thermique_C 340 5-7_Left_FR-FR" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBOILER)
    Phase Created = "3. New Construction" (IFCLABEL)
  Visibility | properties | on 1 object (1 IFCBOILER)
    Control Unit on Back = FALSE (IFCBOOLEAN)
    Control Unit on Side = TRUE (IFCBOOLEAN)
    Optional Connection = TRUE (IFCBOOLEAN)
    Show Service Space = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Electrical | properties | on 1 type object
    Phase = 1 (IFCINTEGER)
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materials and Finishes | properties | on 1 type object
    Blue = "Color RGB 075-186-252" (IFCLABEL)
    Glass = "Color RGB 218-227-224" (IFCLABEL)
    Grey = "Color RAL 7016" (IFCLABEL)
    Light Gray = "Color RGB 145-145-145" (IFCLABEL)
    Logo = "Color RGB 165-173-178" (IFCLABEL)
    Red = "Color RAL 2002" (IFCLABEL)
    White = "Color RGB 219-219-219" (IFCLABEL)
    Yellow = "Color RGB 255-255-000" (IFCLABEL)
  Text | properties | on 1 type object
    Pipe Type Category = "M561" (IFCTEXT)