IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2016-02-02T12:18:32"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 2014.0.2013.1024 - Default UI"
Application: "Autodesk Revit MEP 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit MEP 2014 (ENU)"

People and organizations
  Person "CN" of Organization (no name given)
  Owner history of Person "CN" of Organization (no name given) | application "Autodesk Revit MEP 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit MEP 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "C 330-570 VD" | object type "C 330-570 VD" | names: "HC_Boiler_MEPcontent_De Dietrich Thermique_C330 ECO VD:C 330-570 VD:667467" | material: materials ("Color RAL 9016", "Color RAL 7016", "Color RAL 7004", "Color RGB 075-186-252", "Color RAL 2002", "Color RAL 1003") | property sets: Other, Constraints, Electrical - Loads, Mechanical, Identity Data, Mechanical - Flow

Types
  IFCBOILERTYPE "C 330-570 VD" | element type "C 330-570 VD" | WATER | 1 occurrence | material: materials ("Color RAL 9016", "Color RAL 7016", "Color RAL 7004", "Color RGB 075-186-252", "Color RAL 2002", "Color RAL 1003")

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Control Unit On Back = FALSE (IFCBOOLEAN)
    Control Unit On Side = TRUE (IFCBOOLEAN)
    Show Service Area = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Auxiliary Hydronic Return Diameter = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 80. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Apparent Load = 0. (IFCREAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Voltage = 2475.69939584324 (IFCREAL)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Drain Fixture Units = 0. (IFCREAL)
    Flow Auxiliary Hydronic Return = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Flue Gas = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Gas = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Hydronic Return = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Hydronic Supply = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Hydronic Supply,Hydronic Return,Other,Supply Air,Other,Sanitary,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Nominal Power = 6178484.57919138 (IFCREAL)
    Tap Capacity at 60°C = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Volume = 3.28426400509844 (IFCREAL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Function Code = "" (IFCTEXT)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Article Description = "Standing boiler with integrated burner" (IFCTEXT)
    Article Type = "C 330-570 VD" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Content Supplier URL = "www.mepcontent.eu" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Cost = 0. (IFCREAL)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Standing boiler with integrated burner" (IFCTEXT)
    EMCS Version = "2.0" (IFCTEXT)
    ETIM Article Class = "EC011396" (IFCTEXT)
    Family Version = "10.06" (IFCTEXT)
    GTIN = "3661238564909" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Language = "" (IFCTEXT)
    MEPcontent Class = "BOILER" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer Art. No. = "100019554" (IFCTEXT)
    Manufacturer URL = "http://www.dedietrich-thermique.fr/produits/gammes_de_produits/chaudieres_grande_puissance/gaz_a_condensation_c" (IFCTEXT)
    Model = "C 330-570 VD" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)
    Revit Version = "2014" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Flow Supply Air = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    A = 2142. (IFCLENGTHMEASURE) [MILLI METRE]
    B = 1944. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Gas Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
    L = 1800. (IFCLENGTHMEASURE) [MILLI METRE]
    Supply Air Diameter = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 716. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Anthracite = "Color RAL 7016" (IFCLABEL)
    Blue = "Color RGB 075-186-252" (IFCLABEL)
    Glass = "Color RGB 218-227-224" (IFCLABEL)
    Grey = "Color RAL 7004" (IFCLABEL)
    Red = "Color RAL 2002" (IFCLABEL)
    White = "Color RAL 9016" (IFCLABEL)
    Yellow = "Color RAL 1003" (IFCLABEL)