IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2016-02-02T12:14:12"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20131024_2115(x64) - Exporter 2014.0.2013.1024 - Default UI"
Application: "Autodesk Revit MEP 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit MEP 2014 (ENU)"

People and organizations
  Person "CN" of Organization (no name given)
  Owner history of Person "CN" of Organization (no name given) | application "Autodesk Revit MEP 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit MEP 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "170" | object type "170" | names: "HC_Boiler_MEPcontent_De Dietrich Thermique_C230 ECO:170:665875" | material: materials ("Color RAL 1003", "Color RAL 7004", "Color RAL 7016", "Color RGB 169-241-116", "Color RAL 9016", "Color RAL 100-100-100") | property sets: Mechanical, Phasing, Identity Data, Constraints, Electrical - Loads, Visibility

Types
  IFCBOILERTYPE "170" | element type "170" | WATER | 1 occurrence | material: materials ("Color RAL 1003", "Color RAL 7004", "Color RAL 7016", "Color RGB 169-241-116", "Color RAL 9016", "Color RAL 100-100-100")

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Flow Auxiliary Hydronic Return = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Flue Gas = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Gas = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Hydronic Return = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Hydronic Supply = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Classification = "Sanitary,Hydronic Return,Hydronic Supply,Hydronic Return,Other,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Fixture Units Drain = 0. (IFCREAL)
    Nominal Power = 1926739.96459104 (IFCREAL)
    Volume = 0.706293334429772 (IFCREAL)
  Phasing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Function Code = "" (IFCTEXT)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Article Description = "Standing boiler with integrated burner" (IFCTEXT)
    Article Type = "170" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Content Supplier URL = "www.mepcontent.eu" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Standing boiler with integrated burner" (IFCTEXT)
    EMCS Version = "2.0" (IFCTEXT)
    ETIM Article Class = "EC011396" (IFCTEXT)
    Family Version = "10.06" (IFCTEXT)
    GTIN = "3661238338586" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    Language = "" (IFCTEXT)
    MEPcontent Class = "BOILER" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer Art. No. = "100010399" (IFCTEXT)
    Manufacturer URL = "http://www.dedietrich-thermique.fr/produits/gammes_de_produits/chaudieres_grande_puissance/gaz_a_condensation_c" (IFCTEXT)
    Model = "170" (IFCTEXT)
    OmniClass Number = "23.75.10.11.14" (IFCTEXT)
    OmniClass Title = "Hot Water Heat Generators" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)
    Revit Version = "2014" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Apparent Load = 2217.3655458422 (IFCREAL)
    Voltage = 2475.72 (IFCREAL)
  Visibility | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Show Service Area = FALSE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Drain Diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1309. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1190. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
    Width = 450. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Flue Gas Diameter = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Height1 = 1272. (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Return Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hydronic Supply Diameter = 31.8 (IFCLENGTHMEASURE) [MILLI METRE]
  Materials and Finishes | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Anthracite = "Color RAL 7016" (IFCLABEL)
    Dusty Grey = "Color RAL 100-100-100" (IFCLABEL)
    Glass = "Color RGB 218-227-224" (IFCLABEL)
    Green = "Color RGB 169-241-116" (IFCLABEL)
    Grey = "Color RAL 7004" (IFCLABEL)
    White = "Color RAL 9016" (IFCLABEL)
    Yellow = "Color RAL 1003" (IFCLABEL)