IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project nummer"
Time stamp: "2018-10-08T11:35:07"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160720_1515(x64) - Exporter 17.0.501.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "FCiofle" of Organization (no name given)
  Owner history of Person "FCiofle" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1538987414 (2018-10-08T08:30:14Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project nummer" | long name "Project omschrijving" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 23′ 13.199999″ | longitude -71° 14′ 31.199999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here"
      IFCBUILDINGSTOREY "V00" | long name "V00" | elevation 0.
        contains 1 element
          1 x IFCTANK | type IFCTANKTYPE "PSB 1000 HR" | object type "PSB 1000 HR" | names: "HC_Storage Tank _MEPcontent_De Dietrich Thermique_FR-EN:PSB 1000 HR:1311420" | material: materials ("Color RGB 246-246-246", "Color RGB 045-045-045") | property sets: Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical, Mechanical - Flow

Types
  IFCTANKTYPE "PSB 1000 HR" | 1 occurrence | material: materials ("Color RGB 246-246-246", "Color RGB 045-045-045") | property sets: Dimensions, Identity Data, Materials and Finishes, Mechanical, Other, Text

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Klant naam" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Aanvraag datum" (IFCTEXT)
    Project Name = "Project omschrijving" (IFCTEXT)
    Project Number = "Project nummer" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCTANK)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "HC_Storage Tank _MEPcontent_De Dietrich Thermique_FR-EN: PSB 1000 HR" (IFCLABEL)
    Family and Type = "HC_Storage Tank _MEPcontent_De Dietrich Thermique_FR-EN: PSB 1000 HR" (IFCLABEL)
    Type = "HC_Storage Tank _MEPcontent_De Dietrich Thermique_FR-EN: PSB 1000 HR" (IFCLABEL)
    Type Id = "HC_Storage Tank _MEPcontent_De Dietrich Thermique_FR-EN: PSB 1000 HR" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Floor Level" (IFCLABEL)
    Family and Type = "Level: Floor Level" (IFCLABEL)
    Type = "Level: Floor Level" (IFCLABEL)
    Type Id = "Level: Floor Level" (IFCLABEL)
  Other | properties | on 1 type object
    Boiler Sensor Position = 22.5 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Bottom Geometry = 47.8444444444444 (IFCLENGTHMEASURE) [MILLI METRE]
    Cap Void 1 = 505. (IFCLENGTHMEASURE) [MILLI METRE]
    Cap Void 2 = 525. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    DCW Pos = 525. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Nominal Diameter 1 = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Nominal Diameter 2 = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Nominal Diameter 3 = 38.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Nominal Diameter 4 = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Outer Diameter 1 = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Outer Diameter 2 = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Outer Diameter 3 = 48.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Outer Diameter 4 = 60.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Family Name = "HC_Storage Tank _MEPcontent_De Dietrich Thermique_FR-EN" (IFCTEXT)
    Holes Distance = 395. (IFCLENGTHMEASURE) [MILLI METRE]
    Tank Radius = 465. (IFCLENGTHMEASURE) [MILLI METRE]
    Tank Rail Diameter = 994.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Geometry = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Floor Level" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCTANK)
    Function Code = "" (IFCTEXT)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "V00" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Article Type = "PSB 1000 HR" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Base Family Version = "11.19" (IFCTEXT)
    CB-NL Class = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Content Supplier URL = "www.MEPcontent.com" (IFCTEXT)
    Copyright = "© Stabiplan International BV" (IFCTEXT)
    Custom = FALSE (IFCBOOLEAN)
    Description = "Storage tank indoor unit" (IFCTEXT)
    EMCS Version = "4.0" (IFCTEXT)
    ETIM Article Class = "EC010184" (IFCTEXT)
    Family Version = "11.19" (IFCTEXT)
    GLN = "" (IFCTEXT)
    Internal Art. No. = "" (IFCTEXT)
    MEPcontent Class = "STORAGE_TANK_HC" (IFCTEXT)
    Manufacturer = "De Dietrich Thermique" (IFCTEXT)
    Manufacturer URL = "https://www.dedietrich-thermique.fr/" (IFCTEXT)
    Model = "PSB 1000 HR" (IFCTEXT)
    OmniClass Number = "23.75.10.34.11" (IFCTEXT)
    OmniClass Title = "Energy Storage Tanks" (IFCTEXT)
    Revit Version = "2017" (IFCTEXT)
    Stabu Code = "" (IFCTEXT)
    Type Name = "PSB 1000 HR" (IFCTEXT)
    URL = "www.stabiplan.com" (IFCTEXT)
    Watermarked By = "www.stabiplan.com" (IFCTEXT)
    Wholesaler = "" (IFCTEXT)
    Wholesaler Art. No. = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "GE_tag_level_floor_MEPcontent: standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCTANK)
    Manufacturer = "De Dietrich Thermique" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCTANK)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    S4R_Use_nominal_diameter = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 1 object (1 IFCTANK)
    Area = 4.3575355041595 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.73544493808433 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    A = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    B = 420. (IFCLENGTHMEASURE) [MILLI METRE]
    C = 905. (IFCLENGTHMEASURE) [MILLI METRE]
    D = 1845. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter = 990. (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter 1 = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter 2 = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter 3 = 38.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Domestic Hot Water Diameter 4 = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    E = 2115. (IFCLENGTHMEASURE) [MILLI METRE]
    F = 1134. (IFCLENGTHMEASURE) [MILLI METRE]
    G = 115. (IFCLENGTHMEASURE) [MILLI METRE]
    H1 = 2153. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2253. (IFCLENGTHMEASURE) [MILLI METRE]
    Use Nominal Diameter = TRUE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCTANK)
    System Classification = "Domestic Hot Water,Communication,Domestic Hot Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Maximum Operating Pressure (bar) = 5. (IFCREAL)
    Maximum Temperature (°C) = "95" (IFCTEXT)
    Volume = 1000. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Mechanical - Flow | properties | on 1 object (1 IFCTANK)
    Domestic Hot Water Flow 1 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 2 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 3 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 4 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 5 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 6 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 7 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Domestic Hot Water Flow 8 = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCTANK)
    Phase Created = "4. Plan over 10 jaar" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    Black = "Color RGB 045-045-045" (IFCLABEL)
    Grey = "Color RGB 165-165-165" (IFCLABEL)
    White = "Color RGB 246-246-246" (IFCLABEL)
  Text | properties | on 1 type object
    Article Description = "Storage tank indoor unit" (IFCTEXT)
    GTIN = "" (IFCTEXT)
    Manufacturer Art. No. = "" (IFCTEXT)
    Product Line = "De Dietrich Thermique" (IFCTEXT)